SEEN Operator Station & Equipment Details|F!702

# Revision 02-22-2025 - SEEN

! This is a SEEN JS8Spotter MCForms form.

? Station activity level on JS8Call (attended or unattended):
@1 Station attempts to operate 24/7
@2 Station operates daily on a schedule
@3 Station operates daily as available
@4 Station operates weekly
@5 Station operates only incidentially

? Station max RF power capability:
@1 QRP 0-5W
@2 5-10W
@3 10-50W
@4 100W
@5 300-500W amplified
@6 Over 500W amplified
@7 Legal limit amplified

? Primary HF antenna (antenna with longest range and most reliable operation):
@1 Operating portable at this time
@2 Center-Fed Dipole
@3 End Fed Half Wave
@4 Loop
@5 Beam - tower mount
@9 Other

? Additional antennas:
@1 Yes, additional antennas 
@2 No additional antennas 

? Bands and modes actively operated at primary station:
@1 All HF bands, all modes, including CW
@2 All HF bands, all modes, no CW 

? Digital modes configured (select the best match to your setup):
@1 JS8Call, + all modes supported by FLDigi + Winlink, VARAC
@2 JS8Call, + all modes supported by FLDigi + Winlink
@3 JS8Call, + all modes supported by FLDigi
@4 JS8Call, + Winlink, VARAC
@5 JS8Call, + VARAC

? Grid down capabilities:
@1 Battery capacity for at least 24hrs of continuous low-duty-cycle operating time, solar charging available
@2 Battery capacity for at least 48hrs of continuous low-duty-cycle operating time, solar charging available
@3 Battery capacity for at least 72hrs of continuous low-duty-cycle operating time, solar charging available
@4 Battery capacity for at least 24hrs of continuous low-duty-cycle operating time, no off-grid charging ability
@5 Battery capacity for at least 48hrs of continuous low-duty-cycle operating time, no off-grid charging ability
@6 Battery capacity for at least 72hrs of continuous low-duty-cycle operating time, no off-grid charging ability
@7 Limited (0-23hrs) or no battery capacity
@8 Whole house generator with battery backup and off-grid charging ability

? Your most active band for JS8Call:
@1 All SEEN and AmRRON frequencies 
@2 160m / 1.842 MHz
@3 80m / 3.578 MHz
@4 40m / 7.078 MHz
@5 30m / 10.130 MHz
@6 20m / 14.078 MHz
@8 17m / 18.104 MHz
@9 15m / 21.078 MHz
@0 12m / 24.922 MHz
@A 10m / 28.078 MHz
@B 6m / 50.318 MHz
@C 2m / 144.178 MHz

? Are you comfortable with allowing other stations to use your system for relays and message store?
@1 Yes
@2 No





